* Basics:
	+ Only 1 plane at a time.
	+ Check the small box at the bottom on the left, which is the auto-save.
	+ For today’s beam (1380, ~ 1.2E11 p/b):
		- Acquisition windows = 100 micros.
		- Sum-Signal Scale = 500 mV.
		- Delta-Signal Scale = 100 mV.
* Triggering on BBQ (threshold mechanism):
	+ In Configure, de-check the “force scope trigger”.
	+ Open firefox on an xterm and go to cfo-ua47-bqhttrig.cern.ch.
	+ De-check the 2 boxes called “Force TTL trigger B1 and B2 + Set. If does not work, change in the url to have the Trigger 0 = 0 and 1 = 0.
	+ Now, the HEADTAIL monitor is waiting for a trigger from the BBQ, which will come when the signal will reach there ~ 30% of the maximum (set by Ralph, 338 bins out of 1023).
	+ To stop the acquisition it is sometimes better to re-click on the Acquisition button instead of the stop.
	+ Put back the trigger (see 3rd bullet.)