* Basics:
  + Only 1 plane at a time.
  + Check the small box at the bottom on the left, which is the auto-save.
  + For today’s beam (1380, ~ 1.2E11 p/b):
    - Acquisition windows = 100 micros.
    - Sum-Signal Scale = 500 mV.
    - Delta-Signal Scale = 100 mV.
* Triggering on BBQ (threshold mechanism):
  + In Configure, de-check the “force scope trigger”.
  + Open firefox on an xterm and go to cfo-ua47-bqhttrig.cern.ch.
  + De-check the 2 boxes called “Force TTL trigger B1 and B2 + Set. If does not work, change in the url to have the Trigger 0 = 0 and 1 = 0.
  + Now, the HEADTAIL monitor is waiting for a trigger from the BBQ, which will come when the signal will reach there ~ 30% of the maximum (set by Ralph, 338 bins out of 1023).
  + To stop the acquisition it is sometimes better to re-click on the Acquisition button instead of the stop.
  + Put back the trigger (see 3rd bullet.)